<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="38.151" y2="0" width="0" layer="20"/>
<wire x1="38.151" y1="0" x2="38.278" y2="39.233" width="0" layer="20"/>
<wire x1="38.278" y1="39.233" x2="0" y2="39.36" width="0" layer="20"/>
<wire x1="0" y1="39.36" x2="0" y2="0" width="0" layer="20"/>
<text>DS003B</text>
<text>C2018 Geo</text>
<text>1</text>
<text>2</text>
</plain>
<libraries>
<library name="mylib">
<description>&lt;p&gt;Moje elementy dla projektów &lt;b&gt;Eagle&lt;/b&gt;&lt;/p&gt;</description>
<packages>
<package name="SML0805">
<description>&lt;b&gt;SML0805-2CW-TR (0805 PROFILE)&lt;/b&gt; COOL WHITE&lt;p&gt;
Source: http://www.ledtronics.com/ds/smd-0603/Dstr0093.pdf</description>
</package>
<package name="1X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X05">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="R0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Switches">
<description>&lt;h3&gt;SparkFun Switches, Buttons, Encoders&lt;/h3&gt;
In this library you'll find switches, buttons, joysticks, and anything that moves to create or disrupt an electrical connection.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TACTILE_SWITCH_SMD_6.0X3.5MM">
<description>&lt;h3&gt;Momentary Switch (Pushbutton) - SPST - SMD, 6.0 x 3.5 mm&lt;/h3&gt;
&lt;p&gt;Normally-open (NO) SPST momentary switches (buttons, pushbuttons).&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.sparkfun.com/datasheets/Components/1101.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="D1" library="mylib" package="SML0805" value="">
<attribute name="VALUE"/>
</element>
<element name="D10" library="mylib" package="SML0805" value="">
<attribute name="VALUE"/>
</element>
<element name="D12" library="mylib" package="SML0805" value="">
<attribute name="VALUE"/>
</element>
<element name="D11" library="mylib" package="SML0805" value="">
<attribute name="VALUE"/>
</element>
<element name="D2" library="mylib" package="SML0805" value="">
<attribute name="VALUE"/>
</element>
<element name="D3" library="mylib" package="SML0805" value="">
<attribute name="VALUE"/>
</element>
<element name="D4" library="mylib" package="SML0805" value="">
<attribute name="VALUE"/>
</element>
<element name="D5" library="mylib" package="SML0805" value="">
<attribute name="VALUE"/>
</element>
<element name="D6" library="mylib" package="SML0805" value="">
<attribute name="VALUE"/>
</element>
<element name="D7" library="mylib" package="SML0805" value="">
<attribute name="VALUE"/>
</element>
<element name="D8" library="mylib" package="SML0805" value="">
<attribute name="VALUE"/>
</element>
<element name="D9" library="mylib" package="SML0805" value="">
<attribute name="VALUE"/>
</element>
<element name="JP1" library="mylib" package="1X03" value="">
<attribute name="VALUE"/>
</element>
<element name="JP2" library="mylib" package="1X05" value="">
<attribute name="VALUE"/>
</element>
<element name="R0" library="mylib" package="R0805" value="220">
<attribute name="SPICEPREFIX" value="R"/>
</element>
<element name="R1" library="mylib" package="R0805" value="220">
<attribute name="SPICEPREFIX" value="R"/>
</element>
<element name="R2" library="mylib" package="R0805" value="220">
<attribute name="SPICEPREFIX" value="R"/>
</element>
<element name="R3" library="mylib" package="R0805" value="220">
<attribute name="SPICEPREFIX" value="R"/>
</element>
<element name="W" library="SparkFun-Switches" package="TACTILE_SWITCH_SMD_6.0X3.5MM" value="MOMENTARY-SWITCH-SPST-SMD-6.0X3.5MM">
<attribute name="PROD_ID" value="SWCH-00815"/>
<attribute name="SF_SKU" value="COM-08229"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="JP1" pad="2"/>
<contactref element="W" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="R2" pad="1"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="N$4">
<contactref element="R1" pad="1"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="R0" pad="1"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="D12" pad="C"/>
<contactref element="R3" pad="2"/>
<contactref element="D10" pad="C"/>
<contactref element="D9" pad="A"/>
<contactref element="D11" pad="A"/>
<contactref element="D5" pad="A"/>
<contactref element="D6" pad="C"/>
</signal>
<signal name="N$7">
<contactref element="D12" pad="A"/>
<contactref element="R0" pad="2"/>
<contactref element="D7" pad="C"/>
<contactref element="D8" pad="A"/>
<contactref element="D11" pad="C"/>
<contactref element="D2" pad="A"/>
<contactref element="D1" pad="C"/>
</signal>
<signal name="N$8">
<contactref element="D8" pad="C"/>
<contactref element="R2" pad="2"/>
<contactref element="D7" pad="A"/>
<contactref element="D5" pad="C"/>
<contactref element="D6" pad="A"/>
<contactref element="D4" pad="C"/>
<contactref element="D3" pad="A"/>
</signal>
<signal name="N$9">
<contactref element="R1" pad="2"/>
<contactref element="D10" pad="A"/>
<contactref element="D9" pad="C"/>
<contactref element="D3" pad="C"/>
<contactref element="D4" pad="A"/>
<contactref element="D2" pad="C"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="N$1">
<contactref element="R3" pad="1"/>
<contactref element="JP2" pad="4"/>
</signal>
<signal name="N$2">
<contactref element="W" pad="1"/>
<contactref element="JP2" pad="5"/>
</signal>
<signal name="N$10">
</signal>
</signals>
</board>
</drawing>
</eagle>
